# Main Loop

The main loop uses the function named get\_command to retrieve characters from the serial port.

The function named get\_command contains a while loop in which the serial is queried via a call to MSerial.available().

Each character from the serial port is saved to the buffer named cmdbuffer. This buffer is a 2 dimensional array: 4(BUFSIZE) x 96(MAX\_CMD\_SIZE).